Debug:(toolbox.cpp:72, ) ToolBox Start.....
Debug:(:0, ) QObject::connect: No such signal LogWnd::close()
Debug:(:0, ) QObject::connect:  (sender name:   'LogWnd')
Debug:(:0, ) QObject::connect:  (receiver name: 'LogWnd')
Debug:(toolbox.cpp:1855, ) "C:/Users/admin/Desktop/ToolBox/translations/ToolBox_zh_CN.qm"
Debug:(lorawanpage.cpp:307, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:185, ) m_loraReadIndex: 945688 false false
Debug:(qunpbasic.cpp:1941, ) false "COM12" "COM12"
Debug:(qnfcbasic.cpp:1016, ) [ACK LEN] 1926 [ACK DATA] "4d3c2b1a785634120100860700000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000055"
Debug:(qnfcbasic.cpp:1024, ) ===recv_len = 1926, recv_num = 31
Debug:(qnfcbasic.cpp:1040, ) [recv:]  " "
Debug:(qunpbasic.cpp:2134, ) connecting unp_get_product_name... UC501 
Debug:(qunpbasic.cpp:2140, ) connectting... m_product  "UC501"
Debug:(qunpbasic.cpp:2169, ) pn--- -470M

Debug:(qnfcbasic.cpp:189, ) product... "UC501" "-470M" "3.0" 256
Debug:(qnfcbasic.cpp:193, ) "UC501" 256
Debug:(qnfcbasic.cpp:194, ) ## imagesize: 1926

Debug:(qnfcbasic.cpp:195, ) ############# 682679b0

Debug:(qnfcbasic.cpp:196, ) ############# 61526f4c

Debug:(qunpbasic.cpp:1941, ) true "COM12" "COM12"
Debug:(qnfcbasic.cpp:1016, ) [ACK LEN] 1926 [ACK DATA] "4d3c2b1a785634120100860700000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000055"
Debug:(qnfcbasic.cpp:1024, ) ===recv_len = 1926, recv_num = 31
Debug:(qnfcbasic.cpp:1040, ) [recv:]  " "
Debug:(qunpbasic.cpp:2134, ) connecting unp_get_product_name... UC501 
Debug:(qunpbasic.cpp:2140, ) connectting... m_product  "UC501"
Debug:(qunpbasic.cpp:2169, ) pn--- -470M

Debug:(qnfcbasic.cpp:242, ) product... "UC501" "-470M" "3.0" 0
Debug:(qnfcbasic.cpp:246, ) "UC501" 0
Debug:(qnfcbasic.cpp:247, ) ## imagesize: 1926

Debug:(qnfcbasic.cpp:248, ) ############# 682679b0

Debug:(qnfcbasic.cpp:249, ) ############# 682679b0

Debug:(connectting.cpp:236, ) Device Connect Success
Debug:(qunpbasic.cpp:2134, ) connecting unp_get_product_name... UC501 
Debug:(qunpbasic.cpp:2140, ) connectting... m_product  "UC501"
Debug:(qunpbasic.cpp:2169, ) pn--- -470M

Debug:(qunpbasic.cpp:2326, ) pn3--- 

Debug:(connectting.cpp:269, ) product name pn:  "UC501--470M"
Debug:(connectting.cpp:285, ) close serial port
Debug:(toolbox.cpp:392, ) product name: "UC501--470M" "" "01.06" "3.0" 0 86
Debug:(uc50xv3dealthread.cpp:19, ) Thread id: 0xe2c
Debug:(uc50xv3dealthread.cpp:117, ) request type:0
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101050000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:156, ) "UC501" UC501 0
Debug:(qnfcuc50xv3.cpp:160, ) ## imagesize: 1926

Debug:(qnfcuc50xv3.cpp:161, ) ############# e279c322

Debug:(qnfcuc50xv3.cpp:162, ) ############# e279c322

Debug:(qunpuc50xv3.cpp:3940, ) oemName--- 

Debug:(qunpuc50xv3.cpp:3962, ) oempn--- 

Debug:(qunpuc50xv3.cpp:621, ) ===== -470M
Debug:(qunpuc50xv3.cpp:2115, ) pn--- 470M

Debug:(uc50xv3dealthread.cpp:380, ) "UC501-470M"
Debug:(qunpuc50xv3.cpp:631, ) ===device oem:0086

Debug:(qunpuc50xv3.cpp:2212, ) pn3--- 

Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 11 len 8

Debug:(uc50xv3dealthread.cpp:117, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 214 len 1

Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 0 len 106

Debug:(uc50xv3dealthread.cpp:604, ) appPort0000: "85" 0 0
Debug:(uc50xv3generalpage.cpp:2403, ) 
Debug:(uc50xv3generalpage.cpp:2403, ) 
Debug:(ucchannelv3Page.cpp:30, ) onAddActionCmdSlot... 1
Debug:(uc50xv3generalpage.cpp:1341, ) "UC501-470M" "3.0"
Debug:(uc50xv3dealthread.cpp:117, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3generalpage.cpp:1341, ) "UC501-470M" "3.0"
Debug:(uc50xv3dealthread.cpp:117, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:402, ) 3 1
Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a7856341201020e0000000031323334353603010000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(qnfcuc50xv3.cpp:1160, ) after send connect data

Debug:(uc50xv3dealthread.cpp:117, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 214 len 1

Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 0 len 106

Debug:(uc50xv3dealthread.cpp:604, ) appPort0000: "85" 0 0
Debug:(uc50xv3generalpage.cpp:2403, ) 
Debug:(uc50xv3generalpage.cpp:2403, ) 
Debug:(ucchannelv3Page.cpp:30, ) onAddActionCmdSlot... 1
Debug:(uc50xv3dealthread.cpp:117, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3generalpage.cpp:1341, ) "UC501-470M" "3.0"
Debug:(uc50xv3dealthread.cpp:117, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101060000000000000000000003010000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:192, ) 
Debug:(uc50xv3dealthread.cpp:1084, ) GPIO1 Fetch :
Debug:(uc50xv3dealthread.cpp:1096, ) "1"
Debug:(uc50xv3dealthread.cpp:117, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:402, ) 3 1
Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a7856341201020e0000000031323334353603010000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(qnfcuc50xv3.cpp:1160, ) after send connect data

Debug:(uc50xv3dealthread.cpp:117, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:117, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101060000000000000000000003010000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:192, ) 
Debug:(uc50xv3dealthread.cpp:1084, ) GPIO1 Fetch :
Debug:(uc50xv3dealthread.cpp:1096, ) "1"
Debug:(uc50xv3dealthread.cpp:117, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:402, ) 3 1
Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a7856341201020e0000000031323334353603010000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(qnfcuc50xv3.cpp:1160, ) after send connect data

Debug:(uc50xv3dealthread.cpp:117, ) request type:8
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:692, ) setType: "gpio"
Debug:(uc50xv3dealthread.cpp:760, ) countChange: false false
Debug:(uc50xv3dealthread.cpp:117, ) request type:9
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:217, ) ######calulate_crc = 074d974f

Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a785634120102010607000031323334353600000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(qnfcuc50xv3.cpp:1160, ) after send connect data

Debug:(qnfcuc50xv3.cpp:1166, ) after recv connect data

Debug:(qnfcuc50xv3.cpp:1190, ) recv_buf1 send_num=28  len=1798

Debug:(uc50xv3dealthread.cpp:330, ) 0 0
Debug:(uc50xv3dealthread.cpp:117, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101060000000000000000000003010000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:192, ) 
Debug:(uc50xv3dealthread.cpp:1084, ) GPIO1 Fetch :
Debug:(uc50xv3dealthread.cpp:1096, ) "1"
Debug:(uc50xv3dealthread.cpp:117, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 214 len 1

Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 0 len 106

Debug:(uc50xv3dealthread.cpp:604, ) appPort0000: "85" 0 0
Debug:(uc50xv3generalpage.cpp:2403, ) 
Debug:(uc50xv3generalpage.cpp:2403, ) 
Debug:(ucchannelv3Page.cpp:30, ) onAddActionCmdSlot... 1
Debug:(uc50xv3dealthread.cpp:117, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:117, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:117, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3generalpage.cpp:1341, ) "UC501-470M" "3.0"
Debug:(uc50xv3dealthread.cpp:117, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:402, ) 3 1
Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a7856341201020e0000000031323334353603010000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(qnfcuc50xv3.cpp:1160, ) after send connect data

Debug:(uc50xv3dealthread.cpp:117, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:117, ) request type:8
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:117, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:402, ) 3 2
Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a7856341201020e0000000031323334353603020000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(qnfcuc50xv3.cpp:1160, ) after send connect data

Debug:(uc50xv3dealthread.cpp:117, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101060000000000000000000003020000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:192, ) 
Debug:(uc50xv3dealthread.cpp:1129, ) GPIO2 Fetch :
Debug:(uc50xv3dealthread.cpp:117, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101060000000000000000000003010000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:192, ) 
Debug:(uc50xv3dealthread.cpp:1084, ) GPIO1 Fetch :
Debug:(uc50xv3dealthread.cpp:1096, ) "1"
Debug:(uc50xv3generalpage.cpp:1341, ) "UC501-470M" "3.0"
Debug:(uc50xv3dealthread.cpp:117, ) request type:8
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:692, ) setType: "gpio"
Debug:(uc50xv3dealthread.cpp:760, ) countChange: false false
Debug:(uc50xv3dealthread.cpp:798, ) 0
Debug:(uc50xv3dealthread.cpp:117, ) request type:8
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:692, ) setType: "gpio"
Debug:(uc50xv3dealthread.cpp:760, ) countChange: false false
Debug:(uc50xv3dealthread.cpp:798, ) 0
Debug:(uc50xv3dealthread.cpp:117, ) request type:9
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:217, ) ######calulate_crc = a173f6e2

Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a785634120102010607000031323334353600000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(qnfcuc50xv3.cpp:1160, ) after send connect data

Debug:(qnfcuc50xv3.cpp:1166, ) after recv connect data

Debug:(qnfcuc50xv3.cpp:1190, ) recv_buf1 send_num=28  len=1798

Debug:(uc50xv3dealthread.cpp:330, ) 0 0
Debug:(uc50xv3dealthread.cpp:117, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:117, ) request type:8
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:692, ) setType: "gpio"
Debug:(uc50xv3dealthread.cpp:760, ) countChange: false false
Debug:(uc50xv3dealthread.cpp:798, ) 0
Debug:(uc50xv3dealthread.cpp:117, ) request type:8
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:692, ) setType: "gpio"
Debug:(uc50xv3dealthread.cpp:760, ) countChange: false false
Debug:(uc50xv3dealthread.cpp:798, ) 0
Debug:(uc50xv3dealthread.cpp:117, ) request type:0
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101050000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:156, ) "UC501" UC501 0
Debug:(qnfcuc50xv3.cpp:160, ) ## imagesize: 1926

Debug:(qnfcuc50xv3.cpp:161, ) ############# fabcf0b5

Debug:(qnfcuc50xv3.cpp:162, ) ############# fabcf0b5

Debug:(qunpuc50xv3.cpp:3940, ) oemName--- 

Debug:(qunpuc50xv3.cpp:3962, ) oempn--- 

Debug:(qunpuc50xv3.cpp:621, ) ===== -470M
Debug:(qunpuc50xv3.cpp:2115, ) pn--- 470M

Debug:(uc50xv3dealthread.cpp:380, ) "UC501-470M"
Debug:(qunpuc50xv3.cpp:631, ) ===device oem:0086

Debug:(qunpuc50xv3.cpp:2212, ) pn3--- 

Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 11 len 8

Debug:(uc50xv3dealthread.cpp:117, ) request type:9
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:217, ) ######calulate_crc = fabcf0b5

Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a785634120102010607000031323334353600000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(qnfcuc50xv3.cpp:1160, ) after send connect data

Debug:(qnfcuc50xv3.cpp:1166, ) after recv connect data

Debug:(qnfcuc50xv3.cpp:1190, ) recv_buf1 send_num=28  len=1798

Debug:(uc50xv3dealthread.cpp:330, ) 0 0
Debug:(uc50xv3dealthread.cpp:117, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 214 len 1

Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 0 len 106

Debug:(uc50xv3dealthread.cpp:604, ) appPort0000: "85" 0 0
Debug:(uc50xv3generalpage.cpp:2403, ) 
Debug:(uc50xv3generalpage.cpp:2403, ) 
Debug:(ucchannelv3Page.cpp:30, ) onAddActionCmdSlot... 1
Debug:(uc50xv3dealthread.cpp:117, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3generalpage.cpp:1341, ) "UC501-470M" "3.0"
Debug:(uc50xv3dealthread.cpp:117, ) request type:8
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:117, ) request type:8
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:692, ) setType: "gpio"
Debug:(uc50xv3dealthread.cpp:760, ) countChange: false false
Debug:(uc50xv3dealthread.cpp:798, ) 0
Debug:(uc50xv3dealthread.cpp:810, ) 1
Debug:(uc50xv3dealthread.cpp:117, ) request type:9
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:117, ) request type:8
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:692, ) setType: "gpio"
Debug:(uc50xv3dealthread.cpp:760, ) countChange: false false
Debug:(uc50xv3dealthread.cpp:798, ) 0
Debug:(uc50xv3dealthread.cpp:810, ) 1
Debug:(uc50xv3dealthread.cpp:117, ) request type:9
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:217, ) ######calulate_crc = 100f699f

Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a785634120102010607000031323334353600000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(qnfcuc50xv3.cpp:1160, ) after send connect data

Debug:(qnfcuc50xv3.cpp:1166, ) after recv connect data

Debug:(qnfcuc50xv3.cpp:1190, ) recv_buf1 send_num=28  len=1798

Debug:(uc50xv3dealthread.cpp:330, ) 0 0
Debug:(uc50xv3dealthread.cpp:117, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101060000000000000000000003020000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:192, ) 
Debug:(uc50xv3dealthread.cpp:1539, ) GPIO Counter Fetch : 2
Debug:(uc50xv3dealthread.cpp:1550, ) 
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101080000000000000000000002000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(uc50xv3dealthread.cpp:1576, ) "2" "1"
Debug:(uc50xv3dealthread.cpp:117, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 214 len 1

Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 0 len 106

Debug:(uc50xv3dealthread.cpp:604, ) appPort0000: "85" 0 0
Debug:(uc50xv3generalpage.cpp:2403, ) 
Debug:(uc50xv3generalpage.cpp:2403, ) 
Debug:(ucchannelv3Page.cpp:30, ) onAddActionCmdSlot... 1
Debug:(uc50xv3dealthread.cpp:117, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3generalpage.cpp:1341, ) "UC501-470M" "3.0"
Debug:(uc50xv3generalpage.cpp:1341, ) "UC501-470M" "3.0"
Debug:(uc50xv3generalpage.cpp:1341, ) "UC501-470M" "3.0"
Debug:(uc50xv3generalpage.cpp:1341, ) "UC501-470M" "3.0"
Debug:(uc50xv3dealthread.cpp:117, ) request type:8
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:692, ) setType: "gpio"
Debug:(uc50xv3dealthread.cpp:760, ) countChange: false false
Debug:(uc50xv3dealthread.cpp:810, ) 1
Debug:(uc50xv3dealthread.cpp:117, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101060000000000000000000003020000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:192, ) 
Debug:(uc50xv3dealthread.cpp:1539, ) GPIO Counter Fetch : 2
Debug:(uc50xv3dealthread.cpp:1550, ) 
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101080000000000000000000002000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(uc50xv3dealthread.cpp:1576, ) "2" "1"
Debug:(uc50xv3dealthread.cpp:117, ) request type:9
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:217, ) ######calulate_crc = df461429

Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a785634120102010607000031323334353600000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(qnfcuc50xv3.cpp:1160, ) after send connect data

Debug:(qnfcuc50xv3.cpp:1166, ) after recv connect data

Debug:(qnfcuc50xv3.cpp:1190, ) recv_buf1 send_num=28  len=1798

Debug:(uc50xv3dealthread.cpp:330, ) 0 0
Debug:(uc50xv3generalpage.cpp:1341, ) "UC501-470M" "3.0"
