Debug:(toolbox.cpp:84, ) ToolBox Start.....
Debug:(:0, ) QObject::connect: No such signal LogWnd::close()
Debug:(:0, ) QObject::connect:  (sender name:   'LogWnd')
Debug:(:0, ) QObject::connect:  (receiver name: 'LogWnd')
Debug:(toolbox.cpp:2251, ) "//192.168.5.50/Tftp32/UrsaLink/Images_Test/Toolbox_PC/ToolBox/translations/ToolBox_zh_CN.qm"
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:202, ) m_loraReadIndex: 50845408 false false
Debug:(qunpbasic.cpp:1961, ) false "COM73" "COM73"
Debug:(qnfcbasic.cpp:1199, ) [ACK LEN] 1414 [ACK DATA] "4d3c2b1a785634120100860500000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000055"
Debug:(qnfcbasic.cpp:1207, ) ===recv_len = 1414, recv_num = 23
Debug:(qnfcbasic.cpp:1223, ) [recv:]  " "
Debug:(qnfcbasic.cpp:243, ) "" 0
Debug:(qnfcbasic.cpp:244, ) ## pktsize: 1414

Debug:(qnfcbasic.cpp:245, ) ## flash_size: 1280

Debug:(qnfcbasic.cpp:246, ) ############# a74135ea

Debug:(qnfcbasic.cpp:247, ) ############# a74135ea

Debug:(connectting.cpp:185, ) #####m_flashType: 1
Debug:(connectting.cpp:224, ) Device Connect Success
Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... WS502 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "WS502"
Debug:(qunpbasic.cpp:2190, ) pn--- 470M

Debug:(qunpbasic.cpp:2347, ) pn3--- 2W-W11-CN

Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 11 len 8
Debug:(connectting.cpp:257, ) product name pn:  "WS502-470M"
Debug:(connectting.cpp:288, ) close serial port
Debug:(toolbox.cpp:404, ) product name: "WS502-470M" "2W-W11-CN" "01.01" "1.1" 0 0
Debug:(toolbox.cpp:1001, ) 
Debug:(ws50xdealthread.cpp:19, ) Thread id: 0x6470
Debug:(ws50xdealthread.cpp:121, ) request type:0
Debug:(qunpws50x.cpp:1714, ) false "COM73" "COM73"
Debug:(qunpws50x.cpp:1852, ) pn--- 470M

Debug:(ws50xdealthread.cpp:336, ) swVer::: "01.01"
Debug:(ws50xdealthread.cpp:337, ) rxaxVer::: ""
Debug:(ws50xdealthread.cpp:345, ) "6782C46002131227"
Debug:(qunpws50x.cpp:623, ) ===device oem:

Debug:(qunpws50x.cpp:1962, ) pn3--- 2W-W11-CN

Debug:(qunpws50x.cpp:776, ) read lorawan param:80 pos 11 len 8

Debug:(qunpws50x.cpp:776, ) read lorawan param:80 pos 187 len 58

Debug:(qunpws50x.cpp:776, ) read lorawan param:80 pos 245 len 1

Debug:(ws50xmodel.cpp:2721, ) [单火] true [Class B] false [Class C] false [Class C to B] false false
Debug:(ws50xmodel.cpp:2721, ) [单火] true [Class B] true [Class C] false [Class C to B] false false
Debug:(ws50xmodel.cpp:470, ) [Rx2 freq \ win2Dr ] "505300000" 0 d2denable 0
Debug:(ws50xdealthread.cpp:121, ) request type:1
Debug:(qunpws50x.cpp:1714, ) false "COM73" "COM73"
Debug:(qunpws50x.cpp:776, ) read lorawan param:80 pos 0 len 106

Debug:(ws50xdealthread.cpp:611, ) "ff00" "0" "85"
Debug:(qunpws50x.cpp:776, ) read lorawan param:80 pos 106 len 100

Debug:(qunpws50x.cpp:776, ) read lorawan param:80 pos 215 len 1

Debug:(qunpws50x.cpp:776, ) read lorawan param:80 pos 216 len 1

Debug:(ws50xdealthread.cpp:675, ) info.region**************: "0"
Debug:(qunpws50x.cpp:776, ) read lorawan param:80 pos 214 len 1

Debug:(qunpws50x.cpp:776, ) read lorawan param:80 pos 218 len 1

Debug:(qunpws50x.cpp:776, ) read lorawan param:80 pos 217 len 1

Debug:(qunpws50x.cpp:776, ) read lorawan param:80 pos 96 len 10

Debug:(qunpws50x.cpp:776, ) read lorawan param:80 pos 221 len 1

Debug:(qunpws50x.cpp:776, ) read lorawan param:80 pos 212 len 1

Debug:(qunpws50x.cpp:776, ) read lorawan param:80 pos 222 len 2

Debug:(qunpws50x.cpp:776, ) read lorawan param:80 pos 249 len 200

Debug:(ws50xdealthread.cpp:716, ) group[0] mode:1  devaddr:11111111 
Debug:(ws50xdealthread.cpp:717, ) group[0] mode:0  devaddr:22222222 
Debug:(ws50xdealthread.cpp:718, ) group[0] mode:0  devaddr:33333333 
Debug:(ws50xdealthread.cpp:719, ) group[0] mode:0  devaddr:44444444 
Debug:(ws50xmodel.cpp:1004, ) -1
Debug:(ws50xmodel.cpp:2721, ) [单火] true [Class B] true [Class C] false [Class C to B] false false
Debug:(ws50xmodel.cpp:1032, ) [Rx2 freq ] "505300000" "0"
Debug:(ws50xmodel.cpp:1085, ) mcConfigVer::: 2
Debug:(ws50xmodel.cpp:1388, ) region:  "0"
Debug:(ws50xmodel.cpp:1388, ) region:  "0"
Debug:(ws50xmodel.cpp:1690, ) "1111111111111111" "1111111111111111" "1111111111111111" "1111111111111111" "1111111111111111" "1111111111111111"
Debug:(ws50xmodel.cpp:1693, ) ("0", "1", "2", "3", "4", "5", "6", "7", "8", "9", "10", "11", "12", "13", "14", "15") ("16", "17", "18", "19", "20", "21", "22", "23", "24", "25", "26", "27", "28", "29", "30", "31") ("32", "33", "34", "35", "36", "37", "38", "39", "40", "41", "42", "43", "44", "45", "46", "47") ("48", "49", "50", "51", "52", "53", "54", "55", "56", "57", "58", "59", "60", "61", "62", "63") ("64", "65", "66", "67", "68", "69", "70", "71", "72", "73", "74", "75", "76", "77", "78", "79") ("80", "81", "82", "83", "84", "85", "86", "87", "88", "89", "90", "91", "92", "93", "94", "95")
Debug:(ws50xmodel.cpp:1785, ) (0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 20, 21, 22, 23, 24, 25, 26, 27, 28, 29, 30, 31, 32, 33, 34, 35, 36, 37, 38, 39, 40, 41, 42, 43, 44, 45, 46, 47, 48, 49, 50, 51, 52, 53, 54, 55, 56, 57, 58, 59, 60, 61, 62, 63, 64, 65, 66, 67, 68, 69, 70, 71, 72, 73, 74, 75, 76, 77, 78, 79, 80, 81, 82, 83, 84, 85, 86, 87, 88, 89, 90, 91, 92, 93, 94, 95) ("0-95") 96 1
Debug:(ws50xmodel.cpp:1800, ) ("0-95")
Debug:(ws50xmodel.cpp:1388, ) region:  "0"
Debug:(ws50xmodel.cpp:1690, ) "1111111111111111" "1111111111111111" "1111111111111111" "1111111111111111" "1111111111111111" "1111111111111111"
Debug:(ws50xmodel.cpp:1693, ) ("0", "1", "2", "3", "4", "5", "6", "7", "8", "9", "10", "11", "12", "13", "14", "15") ("16", "17", "18", "19", "20", "21", "22", "23", "24", "25", "26", "27", "28", "29", "30", "31") ("32", "33", "34", "35", "36", "37", "38", "39", "40", "41", "42", "43", "44", "45", "46", "47") ("48", "49", "50", "51", "52", "53", "54", "55", "56", "57", "58", "59", "60", "61", "62", "63") ("64", "65", "66", "67", "68", "69", "70", "71", "72", "73", "74", "75", "76", "77", "78", "79") ("80", "81", "82", "83", "84", "85", "86", "87", "88", "89", "90", "91", "92", "93", "94", "95")
Debug:(ws50xmodel.cpp:1785, ) (0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 20, 21, 22, 23, 24, 25, 26, 27, 28, 29, 30, 31, 32, 33, 34, 35, 36, 37, 38, 39, 40, 41, 42, 43, 44, 45, 46, 47, 48, 49, 50, 51, 52, 53, 54, 55, 56, 57, 58, 59, 60, 61, 62, 63, 64, 65, 66, 67, 68, 69, 70, 71, 72, 73, 74, 75, 76, 77, 78, 79, 80, 81, 82, 83, 84, 85, 86, 87, 88, 89, 90, 91, 92, 93, 94, 95) ("0-95") 96 1
Debug:(ws50xmodel.cpp:1800, ) ("0-95")
Debug:(ws50xmodel.cpp:1690, ) "1111111100000000" "0000000000000000" "0000000000000000" "0000000000000000" "0000000000000000" "0000000000000000"
Debug:(ws50xmodel.cpp:1693, ) ("8", "9", "10", "11", "12", "13", "14", "15") () () () () ()
Debug:(ws50xmodel.cpp:1785, ) (8, 9, 10, 11, 12, 13, 14, 15) ("8-15") 8 1
Debug:(ws50xmodel.cpp:1800, ) ("8-15")
Debug:(basicmethod.cpp:66, ) lora Rx2 Freq Range max min value region 509700000 500300000 505300000 0
Debug:(ws50xdealthread.cpp:121, ) request type:6
Debug:(qunpws50x.cpp:1714, ) false "COM73" "COM73"
Debug:(ws50xdealthread.cpp:745, ) true false false true
Debug:(ws50xdealthread.cpp:1541, ) String to Hex str: "24E124782C460021"
Debug:(qunpws50x.cpp:1061, ) Lora write NFC start_pos: 11  params_len:  8
Debug:(ws50xdealthread.cpp:1541, ) String to Hex str: "24E124C0002A0003"
Debug:(qunpws50x.cpp:1061, ) Lora write NFC start_pos: 19  params_len:  8
Debug:(qunpws50x.cpp:1061, ) Lora write NFC start_pos: 92  params_len:  1
Debug:(ws50xdealthread.cpp:1561, ) String to Hex2 str: "010203"
Debug:(qunpws50x.cpp:1061, ) Lora write NFC start_pos: 3  params_len:  4
Debug:(ws50xdealthread.cpp:1561, ) String to Hex2 str: "00000000"
Debug:(qunpws50x.cpp:1061, ) Lora write NFC start_pos: 7  params_len:  4
Debug:(ws50xdealthread.cpp:1541, ) String to Hex str: "1"
Debug:(qunpws50x.cpp:1061, ) Lora write NFC start_pos: 0  params_len:  1
Debug:(ws50xdealthread.cpp:1541, ) String to Hex str: "2"
Debug:(qunpws50x.cpp:1061, ) Lora write NFC start_pos: 221  params_len:  1
Debug:(qunpws50x.cpp:1061, ) Lora write NFC start_pos: 222  params_len:  1
Debug:(qunpws50x.cpp:1061, ) Lora write NFC start_pos: 91  params_len:  1
Debug:(qunpws50x.cpp:1061, ) Lora write NFC start_pos: 2  params_len:  1
Debug:(qunpws50x.cpp:1061, ) Lora write NFC start_pos: 93  params_len:  1
Debug:(qunpws50x.cpp:1061, ) Lora write NFC start_pos: 186  params_len:  1
Debug:(qunpws50x.cpp:1061, ) Lora write NFC start_pos: 218  params_len:  1
Debug:(qunpws50x.cpp:1061, ) Lora write NFC start_pos: 217  params_len:  1
Debug:(qunpws50x.cpp:1061, ) Lora write NFC start_pos: 191  params_len:  1
Debug:(ws50xdealthread.cpp:1561, ) String to Hex2 str: "1e1e4420"
Debug:(qunpws50x.cpp:1061, ) Lora write NFC start_pos: 187  params_len:  4
Debug:(ws50xdealthread.cpp:1541, ) String to Hex str: "2"
Debug:(qunpws50x.cpp:1061, ) Lora write NFC start_pos: 216  params_len:  1
Debug:(qunpws50x.cpp:1061, ) Lora write NFC start_pos: 1  params_len:  1
Debug:(ws50xdealthread.cpp:1561, ) String to Hex2 str: "11111111"
Debug:(ws50xdealthread.cpp:1561, ) String to Hex2 str: "22222222"
Debug:(ws50xdealthread.cpp:1561, ) String to Hex2 str: "33333333"
Debug:(ws50xdealthread.cpp:1561, ) String to Hex2 str: "44444444"
Debug:(qunpws50x.cpp:2010, ) Lora set Multicast :
Debug:(qunpws50x.cpp:1061, ) Lora write NFC start_pos: 249  params_len:  200
Debug:(ws50xdealthread.cpp:846, ) [set] group[0] mode:0  devaddr:1e4c0ae0 
Debug:(ws50xdealthread.cpp:847, ) [set] group[1] mode:ff  devaddr:ffffff 
Debug:(qunpws50x.cpp:1061, ) Lora write NFC start_pos: 245  params_len:  1
Debug:(qnfcws50x.cpp:218, ) 1286 256 0
Debug:(qnfcws50x.cpp:879, ) len:  1286
Debug:(qnfcws50x.cpp:887, ) 1500
Debug:(qnfcws50x.cpp:614, ) 99
Debug:(qnfcws50x.cpp:807, ) deal_with_nfc_ack satus:  0
Debug:(qnfcws50x.cpp:908, ) recv len:  1286
Debug:(qnfcws50x.cpp:807, ) deal_with_nfc_ack satus:  0
Debug:(qnfcws50x.cpp:807, ) deal_with_nfc_ack satus:  0
Debug:(qnfcws50x.cpp:614, ) 99
Debug:(qnfcws50x.cpp:807, ) deal_with_nfc_ack satus:  0
Debug:(ws50xdealthread.cpp:288, ) 0 1 "123456"
Debug:(ws50xdealthread.cpp:121, ) request type:2
Debug:(qunpws50x.cpp:1714, ) false "COM73" "COM73"
Debug:(qunpws50x.cpp:900, ) [debug]: read PARAM_LED_MODE = 1

Debug:(qunpws50x.cpp:900, ) [debug]: read PARAM_LED_MODE = 1

Debug:(qunpws50x.cpp:2766, ) unp_get_d2d_slave... 
Debug:(qunpws50x.cpp:776, ) read lorawan param:80 pos 245 len 1

Debug:(qunpws50x.cpp:776, ) read lorawan param:80 pos 246 len 1

Debug:(qunpws50x.cpp:776, ) read lorawan param:80 pos 0 len 106

Debug:(qunpws50x.cpp:776, ) read lorawan param:80 pos 187 len 58

Debug:(ws50xmodel.cpp:848, ) classType_cbx name:::: "Class B" false
Debug:(ws50xmodel.cpp:768, ) onAddActionCmdSlot... 1
Debug:(ws50xmodel.cpp:594, ) master d2d enable::: 0
Debug:(ws50xmodel.cpp:599, ) master d2d status: 0 "a111"
Debug:(ws50xmodel.cpp:599, ) master d2d status: 0 "b222"
Debug:(ws50xmodel.cpp:599, ) master d2d status: 0 "c333"
Debug:(ws50xdealthread.cpp:121, ) request type:0
Debug:(qunpws50x.cpp:1714, ) false "COM73" "COM73"
Debug:(qnfcws50x.cpp:614, ) 99
Debug:(qnfcws50x.cpp:807, ) deal_with_nfc_ack satus:  0
Debug:(qnfcws50x.cpp:614, ) 99
Debug:(qnfcws50x.cpp:614, ) 99
Debug:(qnfcws50x.cpp:614, ) 99
Debug:(qnfcws50x.cpp:614, ) 99
Debug:(qnfcws50x.cpp:614, ) 99
Debug:(qnfcws50x.cpp:614, ) 99
Debug:(qnfcws50x.cpp:614, ) 99
Debug:(qnfcws50x.cpp:614, ) 99
Debug:(qnfcws50x.cpp:614, ) 99
Debug:(qnfcws50x.cpp:614, ) 99
Debug:(qnfcws50x.cpp:614, ) 99
Debug:(qnfcws50x.cpp:614, ) 99
Debug:(qnfcws50x.cpp:614, ) 99
Debug:(qnfcws50x.cpp:614, ) 99
Debug:(qnfcws50x.cpp:614, ) 99
Debug:(qnfcws50x.cpp:614, ) 99
Debug:(qnfcws50x.cpp:614, ) 99
Debug:(qnfcws50x.cpp:614, ) 99
Debug:(qnfcws50x.cpp:614, ) 99
Debug:(qnfcws50x.cpp:614, ) 99
Debug:(qnfcws50x.cpp:614, ) 99
Debug:(qnfcws50x.cpp:614, ) 99
Debug:(qnfcws50x.cpp:614, ) 99
Debug:(qnfcws50x.cpp:177, ) ## imagesize: 1414

Debug:(qnfcws50x.cpp:178, ) ############# c7261b6d

Debug:(qnfcws50x.cpp:179, ) ############# c7261b6d

Debug:(qunpws50x.cpp:1852, ) pn--- 470M

Debug:(ws50xdealthread.cpp:336, ) swVer::: "01.01"
Debug:(ws50xdealthread.cpp:337, ) rxaxVer::: ""
Debug:(ws50xdealthread.cpp:345, ) "6782C46002131227"
Debug:(qunpws50x.cpp:623, ) ===device oem:

Debug:(qunpws50x.cpp:1962, ) pn3--- 2W-W11-CN

Debug:(qunpws50x.cpp:776, ) read lorawan param:80 pos 11 len 8

Debug:(qunpws50x.cpp:776, ) read lorawan param:80 pos 187 len 58

Debug:(qunpws50x.cpp:776, ) read lorawan param:80 pos 245 len 1

Debug:(ws50xmodel.cpp:2721, ) [单火] true [Class B] false [Class C] false [Class C to B] false false
Debug:(ws50xmodel.cpp:2721, ) [单火] true [Class B] true [Class C] false [Class C to B] false false
Debug:(ws50xmodel.cpp:470, ) [Rx2 freq \ win2Dr ] "505300000" 0 d2denable 0
