Debug:(toolbox.cpp:84, ) ToolBox Start.....
Debug:(:0, ) QObject::connect: No such signal LogWnd::close()
Debug:(:0, ) QObject::connect:  (sender name:   'LogWnd')
Debug:(:0, ) QObject::connect:  (receiver name: 'LogWnd')
Debug:(toolbox.cpp:2251, ) "C:/Users/admin/Desktop/ToolBox/translations/ToolBox_zh_CN.qm"
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:202, ) m_loraReadIndex: 49304168 false false
Debug:(qunpbasic.cpp:1961, ) false "COM12" "COM12"
Debug:(qnfcbasic.cpp:1199, ) [ACK LEN] 1926 [ACK DATA] "4d3c2b1a785634120100860700000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000055"
Debug:(qnfcbasic.cpp:1207, ) ===recv_len = 1926, recv_num = 31
Debug:(qnfcbasic.cpp:1223, ) [recv:]  " "
Debug:(qnfcbasic.cpp:243, ) "" 0
Debug:(qnfcbasic.cpp:244, ) ## pktsize: 1926

Debug:(qnfcbasic.cpp:245, ) ## flash_size: 1792

Debug:(qnfcbasic.cpp:246, ) ############# c6e859eb

Debug:(qnfcbasic.cpp:247, ) ############# c6e859eb

Debug:(connectting.cpp:185, ) #####m_flashType: 2
Debug:(connectting.cpp:224, ) Device Connect Success
Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... UC501 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "UC501"
Debug:(qunpbasic.cpp:2190, ) pn--- -470M

Debug:(qunpbasic.cpp:2347, ) pn3--- 

Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 11 len 8
Debug:(connectting.cpp:257, ) product name pn:  "UC501--470M"
Debug:(connectting.cpp:288, ) close serial port
Debug:(toolbox.cpp:404, ) product name: "UC501--470M" "" "01.06" "3.0" 0 470
Debug:(uc50xv3dealthread.cpp:20, ) Thread id: 0x4f44
Debug:(uc50xv3dealthread.cpp:118, ) request type:0
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101050000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:156, ) "UC501" UC501 0
Debug:(qnfcuc50xv3.cpp:160, ) ## imagesize: 1926

Debug:(qnfcuc50xv3.cpp:161, ) ############# c6e859eb

Debug:(qnfcuc50xv3.cpp:162, ) ############# c6e859eb

Debug:(qunpuc50xv3.cpp:3940, ) oemName--- 

Debug:(qunpuc50xv3.cpp:3962, ) oempn--- 

Debug:(qunpuc50xv3.cpp:621, ) ===== -470M
Debug:(qunpuc50xv3.cpp:2115, ) pn--- 470M

Debug:(uc50xv3dealthread.cpp:393, ) "UC501-470M"
Debug:(qunpuc50xv3.cpp:631, ) ===device oem:0000

Debug:(qunpuc50xv3.cpp:2212, ) pn3--- 

Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 11 len 8

Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 214 len 1

Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 0 len 106

Debug:(uc50xv3dealthread.cpp:617, ) appPort0000: "85" 0 0
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(ucchannelv3Page.cpp:30, ) onAddActionCmdSlot... 1
Debug:(uc50xv3generalpage.cpp:1360, ) "UC501-470M" "3.0"
Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 214 len 1

Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 0 len 106

Debug:(uc50xv3dealthread.cpp:617, ) appPort0000: "85" 0 0
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(ucchannelv3Page.cpp:30, ) onAddActionCmdSlot... 1
Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3generalpage.cpp:1360, ) "UC501-470M" "3.0"
Debug:(uc50xv3dealthread.cpp:118, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:402, ) 3 1
Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a7856341201020e0000000031323334353603010000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(qnfcuc50xv3.cpp:1160, ) after send connect data

